|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Barrel-1 (13W LED)** | | | **LEGEND** | **QTY** |
|  |  |
| **LOCATION** | *-* | | | |
| **LUMINAIRE DESCRIPTION: Barrel-1 (13W LED) IP65 Surface Mounted Downlight c/w Lamp and Non-Dim Driver.** | | | | |
| **IMAGES / DIMENSIONS** | | | | |
|  | |  | | |
|  | |
| **TECHNICAL SPECIFICATION** | | | | |
| Brand / Model : BARREL-1  Luminous Source : 1 X 13W COB LED  Luminous Output : 1,340 LUMENS PER LUMINAIRE  Color Temperature : 3000K / 4000K / 5000K  Avg Luminous Life : 50,000 BURNING HOURS  Control Gear : INTEGRAL NON-DIM LED DRIVER  Material : ALUMINIUM  Diffuser : CLEAR GLASS COVER  IP Rating : IP 65 | | | | |
|  | | | | |