|  |  |  |
| --- | --- | --- |
| **Barrel-1 (13W LED)** | **LEGEND** | **QTY** |
|  |  |
| **LOCATION** | *-* |
| **LUMINAIRE DESCRIPTION: Barrel-1 (13W LED) IP65 Surface Mounted Downlight c/w Lamp and Non-Dim Driver.** |
| **IMAGES / DIMENSIONS** |
|  |  |
|  |
| **TECHNICAL SPECIFICATION** |
| Brand / Model : BARREL-1Luminous Source : 1 X 13W COB LEDLuminous Output : 1,340 LUMENS PER LUMINAIREColor Temperature : 3000K / 4000K / 5000KAvg Luminous Life : 50,000 BURNING HOURSControl Gear : INTEGRAL NON-DIM LED DRIVERMaterial : ALUMINIUMDiffuser : CLEAR GLASS COVERIP Rating : IP 65 |
|  |